Brighten Academy Promethean and projector installs

Brookmont

**Room 100**

Need Projector Mounted (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to one side of dry erase – may hang over the edge of dry erase. May also need 1” X 4” to make up for depth of dry erase.)

Need Projector Mount

Need 25’ extension cable

Need 25’ vga cable

**Room 102**

Need Projector Mounted (Dell 1510x Projector)

Need Projector Mount

Need 25’ extension cable

Need 25’ vga cable

**Room 106**

Need Projector Rotated 90 Deg. (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to Left side of dry erase – may hang over the edge of dry erase. May also need 1” X 4” to make up for depth of dry erase.)

**Room 205**

Need Projector Mounted (Optomo Projector)

Need Promethean Mounted – ABV378PRO

Need Projector Mount

Need 25’ extension cable

Need 25’ vga cable

**Room 207**

Need Projector Moved (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to one side of dry erase – may hang over the edge of dry erase. May also need 1” X 4” to make up for depth of dry erase.)

Need Projector Mount Pole 2’ (They have a mount without the extension pole)

Prestley Mill Rd

**E137**

Need Projector Mounted (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to Left side of dry erase – may hang over the edge of dry erase. May also need 1” X 4” to make up for depth of dry erase.)

Need Projector Mount

Need Power plug in ceiling above the projector location (to be installed prior to projector install)

Need 25’ vga cable

Cables in wall

Need low voltage cut in

VGA wall plate

VGA gender changer to mount in wall plate

**E137**

Need Projector Mounted (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to Left side of dry erase – may hang over the edge of dry erase. May also need 1” X 4” to make up for depth of dry erase.)

Need Projector Mount Extension pole only - 6”

Need Power plug in ceiling above the projector location (to be installed prior to projector install)

Need 25’ vga cable

**Art**

Need Projector Mounted (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to Left side of dry erase – may hang over the edge of dry erase. May also need 1” X 4” to make up for depth of dry erase.)

Need Projector Mount with 6’ extension pole (This mount will have to mount/clamp to steel. No drop ceiling in this room)

Need Power plug in ceiling above the projector location (to be installed prior to projector install)

Need 45’ vga cable

**E140 – Cafeteria**

Need Projector Mounted (Dell 1510x Projector)

Need Promethean Mounted – ABV378PRO (Mount board to Left side of cork board.)

Need Projector Mount with 4’ extension pole (This mount will have to mount/clamp to steel. No drop ceiling in this room)

Need Power plug in ceiling above the projector location (to be installed prior to projector install)

Need 45’ vga cable